Discuss last weeks work on information propagation. By only allowing major changes during full concensus. Upon reconnect of separated networks, attempt to find last point of consensus. Don’t worry about bad actors since other part of system (permissions) handles that.

Main hub goes down – Everyone disconnected

Part of house loses power – Only part of network disconnects

Two Router Case : Consider later

We should focus on more common errors